================================================================
              CTL100AL Controller Help Information
              FW Version: 2.00.17

/*Help and status commands*/
?/HELP: Print help information.
GET STATUS: Get all status.
/*Commands for system control*/
SET RS232BAUDRATE [a] : Set RS-232 baud rate to a bps.
              a=[0:115200 1:57600, 2:38400, 3:19200, 4:9600]
SET RESET : Reset controller system settings.
SET RESET NETWORK : Reset controller network settings.
SET RESET ALL : Reset controller system and network settings.
              (Type "Yes" To Confirm, "No" To Cancle).
SET REBOOT : Reboot controller.
/*Commands for encoder and decoder control*/
SET ENC PRESET IPMODE [mode] : Preset encoder ip mode.
SET ENC PRESET START IP [ip] : Preset encoder start ip address.
SET ENC PRESET END IP [ip] : Preset encoder end ip address.
SET ENC PRESET GW [gw] : Preset encoder gateway address.
SET ENC PRESET SM [mask] : Preset encoder subnet mask address.
SET ENC PRESET APPLY : Apply the encoder preset ip configuration.
SET ENC [enc] IPMODE DHCP/STATIC : Set the encoder ip mode.
SET ENC [enc] STATIC IP [ip] : Set the encoder static ip address.
SET ENC [enc] STATIC GATEWAY [gw] : Set the encoder static gateway address.
SET ENC [enc] STATIC MASK [mask] : Set the encoder static subnet mask address.
SET ENC [enc] NETWORK REBOOT : Set the encoder network reboot.
SET ENC [enc] LANMODE 1/2 : Set the encoder LAN mode.
SET ENC [enc] LAN2 IPMODE DHCP/STATIC : Set the encoder LAN2 ip mode.SET ENC [enc] LAN2 STATIC IP [ip] : Set the encoder LAN2 static ip address.SET ENC [enc] LAN2 STATIC GATEWAY [gw] : Set the encoder LAN2 static gateway address.SET ENC [enc] LAN2 STATIC MASK [mask] : Set the encoder LAN2 static subnet mask address.SET ENC [enc] ID [id] : Set the index ID of the encoder.
SET ENC [enc] NAME [name] : Set the name of the encoder.
SET ENC [enc] SWITCH [dec] ARC : Set the encoder switch ARC only signals.
              Note: If dec=0, the encoder's signal routing will be closed.
SET ENC [enc] LED ON/OFF : Set the encoder flash power LED or disable flash power LED.
SET ENC [enc] LED ON 90 : Set the encoder flash power LED timeout in 90 seconds.
SET ENC [enc] AUDIO INPUT HDMI/ANA : Set the encoder audio input HDMI or embedded analogue L/R.
SET ENC [enc] EDID COPY [dec] : Set the encoder EDID copy from decoder.
SET ENC [enc] EDID DEFAULT [edid] : Set the encoder Default EDID.
SET ENC [enc] IR VOL 5V/12V : Set the encoder IR voltage 5V or 12V.
SET ENC [enc] IO VOL 5V/12V : Set the encoder IO voltage 5V or 12V.
SET ENC [enc] IO 1 DIR IN/OUT : Set the encoder IO 1 as input or output port.
SET ENC [enc] IO 2 DIR IN/OUT : Set the encoder IO 2 as input or output port.
SET ENC [enc] IO 1 OUT 0/1 : Set the encoder IO 1 output low(0)/high(1) level.
SET ENC [enc] IO 2 OUT 0/1 : Set the encoder IO 2 output low(0)/high(1) level.
SET ENC [enc] RELAY 1 OPEN/CLOSE : Set the encoder relay 1 to open or close.
SET ENC [enc] RELAY 2 OPEN/CLOSE : Set the encoder relay 2 to open or close.
SET ENC [enc] SAC ARC/CEC/OFF : Set the encoder select ARC or CEC or disable ARC and CEC.
SET ENC [enc] NET FIBER/COPPER : Set the encoder network interface.
SET ENC [enc] CEC SEND xx xx : Send CEC data to the encoder, xx is hex data.
SET ENC [enc] IR SEND xxxx xxxx : Send IR data to the encoder, xxxx is hex data.
SET ENC [enc] GUEST ON/OFF BR [br] BIT [bit] : Set the encoder serial guest configuration.
SET ENC [enc] GUEST : Start serial guest mode to encoder.
              Note: To close guest mode use command EXITGUEST.
SET ENC [enc] DELETE : Delete the encoder in the current configuration.
SET ENC [enc] REBOOT : Set the encoder reboot.
SET ENC [enc] RESET : Set the encoder factory reset.
GET ENC [enc] STATUS : Get the encoder status.
SET DEC PRESET IPMODE [mode] : Preset decoder ip mode.
SET DEC PRESET START IP [ip] : Preset decoder start ip address.
SET DEC PRESET END IP [ip] : Preset decoder end ip address.
SET DEC PRESET GW [gw] : Preset decoder gateway address.
SET DEC PRESET SM [mask] : Preset decoder subnet mask address.
SET DEC PRESET APPLY : Apply the decoder preset ip configuration.
SET DEC [dec] IPMODE DHCP/STATIC : Set the decoder ip mode.
SET DEC [dec] STATIC IP [ip] : Set the decoder static ip address.
SET DEC [dec] STATIC GATEWAY [gw] : Set the decoder static gateway address.
SET DEC [dec] STATIC MASK [mask] : Set the decoder static subnet mask address.
SET DEC [dec] NETWORK REBOOT : Set the decoder network reboot.
SET DEC [dec] LANMODE 1/2 : Set the decoder LAN mode.
SET DEC [dec] LAN2 IPMODE DHCP/STATIC : Set the decoder LAN2 ip mode.SET DEC [dec] LAN2 STATIC IP [ip] : Set the decoder LAN2 static ip address.SET DEC [dec] LAN2 STATIC GATEWAY [gw] : Set the decoder LAN2 static gateway address.SET DEC [dec] LAN2 STATIC MASK [mask] : Set the decoder LAN2 static subnet mask address.SET DEC [dec] ID [id] : Set the index ID of the decoder.
SET DEC [dec] NAME [name] : Set the name of the decoder.
SET DEC [dec] SWITCH [enc] ALL : Set the decoder switch all signals.
              Note: If enc=0, the decoder switch to no source.
SET DEC [dec] SWITCH [enc] VIDEO : Set the decoder switch video only signals.
SET DEC [dec] SWITCH [enc] AUDIO : Set the decoder switch audio only signals.
SET DEC [dec] SWITCH [enc] IR : Set the decoder switch IR only signals.
SET DEC [dec] SWITCH [enc] RS232 : Set the decoder switch RS232 only signals.
SET DEC [dec] SWITCH [enc] USB : Set the decoder switch USB only signals.
SET DEC [dec] SWITCH [enc] CEC : Set the decoder switch CEC only signals.
              Note: If enc=0, the decoder's signal routing will return to follow mode.
SET DEC [dec] LED ON/OFF : Set the decoder flash power LED or disable flash power LED.
SET DEC [dec] LED ON 90 : Set the decoder flash power LED timeout in 90 seconds.
SET DEC [dec] OUTPUT ON/OFF : Set the decoder output on or off.
SET DEC [dec] OUTPUT MUTE ON/OFF : Set the decoder output mute on or off.
SET DEC [dec] OUTPUT OSD ON/OFF : Set the decoder output to show ID OSD or hide ID OSD.
SET DEC [dec] OUTPUT RESOLUTION [res] : Set the decoder output resolution.
SET DEC [dec] OUTPUT ROTATE [rtt] : Set the decoder output rotate.
SET DEC [dec] OUTPUT FLIP HOR/VER/OFF : Set the decoder output flip horizontally or vertically.
SET DEC [dec] MODE MX/VW : Set the decoder output mode to matrix or video wall.
SET DEC [dec] IR VOL 5V/12V : Set the decoder IR voltage 5V or 12V.
SET DEC [dec] IO VOL 5V/12V : Set the decoder IO voltage 5V or 12V.
SET DEC [dec] IO 1 DIR IN/OUT : Set the decoder IO 1 as input or output port.
SET DEC [dec] IO 2 DIR IN/OUT : Set the decoder IO 2 as input or output port.
SET DEC [dec] IO 1 OUT 0/1 : Set the decoder IO 1 output low(0)/high(1) level.
SET DEC [dec] IO 2 OUT 0/1 : Set the decoder IO 2 output low(0)/high(1) level.
SET DEC [dec] RELAY 1 OPEN/CLOSE : Set the decoder relay 1 to open or close.
SET DEC [dec] RELAY 2 OPEN/CLOSE : Set the decoder relay 2 to open or close.
SET DEC [dec] ARP ARC/SPDIF : Set the decoder Audio Return Path to ARC or S/PDIF.
SET DEC [dec] EARC DOWNGRADE ON/OFF : Set the decoder eARC downgrade to ARC.
SET DEC [dec] SAC ARC/CEC/OFF : Set the decoder select ARC or CEC or disable ARC and CEC.
SET DEC [dec] NET FIBER/COPPER : Set the decoder network interface.
SET DEC [dec] USB DATA ON/OFF : Set the decoder USB camera enable or disable.
SET DEC [dec] CEC SEND xx xx : Send CEC data to the decoder, xx is hex data.
SET DEC [dec] IR SEND xxxx xxxx : Send IR data to the decoder, xxxx is hex data.
SET DEC [dec] HOTKEY [nn] KEY [k0 k1] ACTION PULL/PUSH SRC [src] : Set the decoder hotkey configuration.
SET DEC [dec] HOTKEY [nn] DEL : Delete the decoder hotkey configuration.
SET DEC [dec] GUEST ON/OFF BR [br] BIT [bit] : Set the decoder serial guest configuration.
SET DEC [dec] GUEST : Start serial guest mode to decoder.
              Note: To close guest mode use command EXITGUEST.
SET DEC [dec] DELETE : Delete the decoder in the current configuration.
SET DEC [dec] REBOOT : Set the decoder reboot.
SET DEC [dec] RESET : Set the decoder factory reset.
GET DEC [dec] STATUS : Get the decoder status.
EXITGUEST : Exit encoder or decoder guest mode.
              dec=0: All decoders
              dec=[1...762]: One decoder
              enc=0: All encoders
              enc=[1...762]: One encoder
              id=[1...762]
              name: max 16 characters
              edid=[00: 1080P,Stereo Audio 2.0 SDR
                    01: 1080P,Dolby/DTS 5.1 SDR
                    02: 1080P,HD Audio 7.1 SDR
                    03: 1080I,Stereo Audio 2.0 SDR
                    04: 1080I,Dolby/DTS 5.1 SDR
                    05: 1080I,HD Audio 7.1 SDR
                    06: 3D,Stereo Audio 2.0 SDR
                    07: 3D,Dolby/DTS 5.1 SDR
                    08: 3D,HD Audio 7.1 SDR
                    09: 4K2K30_444,Stereo Audio 2.0 SDR
                    10: 4K2K30_444,Dolby/DTS 5.1 SDR
                    11: 4K2K30_444,HD Audio 7.1 SDR
                    12: 4K2K60_420,Stereo Audio 2.0 SDR (10/12-bit)
                    13: 4K2K60_420,Dolby/DTS 5.1 SDR (10/12-bit)
                    14: 4K2K60_420,HD Audio 7.1 SDR (10/12-bit)
                    15: 4K2K60_444,Stereo Audio 2.0 SDR (10/12-bit)
                    16: 4K2K60_444,Dolby/DTS 5.1 SDR (10/12-bit)
                    17: 4K2K60_444,HD Audio 7.1 SDR (10/12-bit)
                    18: 4K2K60_444,Stereo Audio 2.0 HDR (10/12-bit)
                    19: 4K2K60_444,Dolby/DTS 5.1 HDR (10/12-bit)
                    20: 4K2K60_444,HD Audio 7.1 HDR (10/12-bit)
                    21: DVI 1280x1024@60Hz, Audio None
                    22: DVI 1920x1080@60Hz, Audio None
                    23: DVI 1920x1200@60Hz, Audio None
                    25: User EDID 1
                    26: User EDID 2]
              res=[00: Bypass
                   01: 1080p@50
                   02: 1080p@60
                   03: 720p@50
                   04: 720p@60
                   05: 2160p@24
                   06: 2160p@30
                   07: 2160p@50
                   08: 2160p@60
                   09: 1280x1024@60
                   10: 1360x768@60
                   11: 1440x900@60
                   12: 1680x1050@60
                   13: 1920x1200@60]
              rtt=[0:0 1:90 2:180 3:270]
              mode=[0:AUTOIP 1:DHCP 2:STATIC]
              br=[0:300   1:600   2:1200  3:2400  4:4800  5:9600]
                 [6:19200 7:38400 8:57600 9:115200]
              bit=Data Bits + Parity + Stop Bits, example: 8n1
                  Data Bits=[5...8], Parity=[n o e], Stop Bits=[1..2]
              ip=[xxx.xxx.xxx.xxx]
              gw=[xxx.xxx.xxx.xxx]
              mask=[xxx.xxx.xxx.xxx]
              nn=[1...20]: Hotkey number
              k0=[01: Left Ctrl
                  02: Right Ctrl
                  03: Left Shift
                  04: Right Shift
                  05: Left Alt
                  06: Right Alt
                  07: Left Shift + Left Ctrl
                  08: Left Ctrl + Left Alt
                  09: Left Shift + Left Alt
              k1=ASCII code
              src=ID of the encoder or decoder
/*Commands for Secondary Stream (SS) control*/
GET ENC [enc] SS STATUS : Get the encoder SS status.
GET ENC [enc] SS MSURL : Get the encoder SS main stream URL.
GET ENC [enc] SS SSURL : Get the encoder SS sub stream URL.
SET ENC [enc] SS REBOOT : Set the encoder SS reboot.
SET ENC [enc] SS RESET : Set the encoder SS factory reset.
SET ENC [enc] SS MAINENCATTR E [etype] H [mhor] V [mver] B [mbr] : Set the encoder SS main stream configuration.
SET ENC [enc] SS SUBENCATTR E [etype] H [shor] V [sver] B [sbr] : Set the encoder SS sub stream configuration.
SET ENC [enc] SS WORKMODE [mode] : Set the encoder SS workMode.
SET ENC [enc] SS NETWORK IP [ip] MASK [mask] GATEWAY [gw] : Set the encoder SS network, can only be used in not follow mode.
SET ENC [enc] SS VLTAG ON [id] : Set the encoder SS vlan tag enable with ID id.
SET ENC [enc] SS VLTAG OFF : Set the encoder SS vlan tag disable.
              enc=0: All encoders
              enc=[1...762]: One encoder
              etype=[0:h264 1:h265]: Encode type
              mhor=[960...1920]: Main stream encode horizontal value(must be even number)
              mver=[540...1080]: Main stream encode vertical value(must be even number)
              shor=[320...960]: Sub stream encode horizontal value(must be even number)
              sver=[180...540]: Sub stream encode vertical value(must be even number)
              mbr=[0...8]: Bit rate (0:1Mb 1:2Mb 2:4Mb 3:6Mb 4:8Mb 5:10Mb 6:12Mb 7:16Mb 8:20Mb)
              sbr=[0...4]: Bit rate (0:128kb 1:256kb 2:512kb 3:1Mb 4:2Mb)
              mode=[0:FOLLOW 1:DHCP 2:STATIC]
              ip=[xxx.xxx.xxx.xxx]
              gw=[xxx.xxx.xxx.xxx]
              mask=[xxx.xxx.xxx.xxx]
              id=[1...4094]: VLAN ID
/*Commands for video wall control*/
CREATE WALL HANDLE [hdl] : Create video wall.
DELETE WALL HANDLE [hdl] : Delete video wall.
SET WALL [hdl] NAME [name] : Set the video wall name.
SET WALL [hdl] C [c] R [r] : Set the video wall columns and rows.
SET WALL [hdl] DEC [dec] H [h] V [v] : Set the video wall position (h,v) decoder.
CREATE WALL [hdl] PRESET [prs] : Create video wall preset.
DELETE WALL [hdl] PRESET [prs] : Delete video wall preset.
SET WALL [hdl] PRESET [prs] NAME [name] : Set the video wall preset name.
APPLY WALL [hdl] PRESET [prs] : Apply video wall preset.
SET WALL [hdl] PRESET [prs] CLASS [cls] H [h] V [v] : Set the video wall preset position (h,v) as class.
SET WALL [hdl] PRESET [prs] CLASS [cls] SOURCE [enc] : Set the video wall preset class from the source.
SET WALL [hdl] PRESET [prs] MATRIX H [h] V [v] : Set the video wall preset to specify the location as a matrix mode.
SET WALL [hdl] PRESET [prs] MATRIX H [h] V [v] SOURCE [enc] : Set the video wall preset class from the source.
SET WALL [hdl] H [h] V [v] WIDTH BEZEL BW [b] IW [i] : Set the video wall position (h,v) base width and image width.
SET WALL [hdl] H [h] V [v] HEIGHT BEZEL BH [b] IH [i] : Set the video wall position (h,v) base height and image height.
GET WALL [hdl] STATUS : Get the video wall Status.
              hdl=[01...09]: Video wall handle
              prs=[01...09]: Preset index
              cls=[A...G]:   Class index
              c=[01...09]: Number of columns in video wall
              r=[01...09]: Number of rows in video wall
              h=[01...09]: Horizontal position in video wall
              v=[01...09]: Vertical position in video wall
              b=[100...1000]: Screen base width/height
              i=[100...1000]: Screen image width/height
              enc=[001...n]: One encoder
              dec=0: Remove decoder from position
              dec=[001...n]: One decoder
              name: Max 16 characters
/*Commands for device management*/
SEARCH : Search all encoders and decoders.
GET SEARCH STATUS : Get the search status.
SEARCH RESET : Reset search encoders and decoders.
ADD DEV [dev] ENC [enc] : Add new encoder devices.
ADD DEV [dev] DEC [dec] : Add new decoder devices.
ADD DEV RESET : Reset all encoders/decoders/videowall/search configurations.
ADD AUTO ALL : Automatically add encoders and decoders for all new searches.
              dev=[01...n]:  Search list index value
              enc=[001...n]: One encoder
              dec=[001...n]: One decoder
/*Commands for GPIO control*/
SET GPIO [gpio] DIR IN/OUT : Set the controller gpio as input or output.
SET GPIO [gpio] LEVEL Low/High : Set the controller gpio output low level or high level.
GET GPIO [gpio] LEVEL : Get the controller gpio input level.
GET GPIO [gpio] STATUS : Get the controller gpio status.
              gpio=00: All IO ports
              gpio=[01...04]: One IO port
/*Commands for network control*/
SET NETWORK [lan] DHCP ON/OFF : Set the controller network dhcp on or off.
SET NETWORK [lan] STATIC IP [ip] : Set the controller network static ip address.
SET NETWORK [lan] STATIC GATEWAY [gw] : Set the controller network static gateway address.
SET NETWORK [lan] STATIC MASK [mask] : Set the controller network static subnet mask address.
SET NETWORK REBOOT : Set the controller network reboot.
SET NETWORK TELNET ON/OFF : Set the controller network telnet on or off.
SET NETWORK TELNET PORT [port] : Set the controller network telnet port.
SET NETWORK SSH ON/OFF : Set the controller network ssh on or off.
SET NETWORK SSH PORT [port] : Set the controller network ssh port.
SET NETWORK HTTPS ON/OFF : Set the controller network https on or off.
SET NETWORK DNS hostname : Set the controller network domain name to hostname.
              lan=LAN1: Video LAN(POE)
              lan=LAN2: Control LAN(Web GUI)
              ip=[xxx.xxx.xxx.xxx]
              gw=[xxx.xxx.xxx.xxx]
              mask=[xxx.xxx.xxx.xxx]
              port=[22...65535]
================================================================

CTL100AL> 